### C-1 Office and Related Commercial District

The purpose of the C-1 office and related commercial district is to provide areas for government offices; professional and *business* offices; medical and dental offices or clinics; *personal care facilities for the elderly*; and *hospitals*, laboratories, *pharmacies* and related complementary *businesses* that provide sales or service of office equipment, medical and dental supplies and office supplies. This district serves as a transitional buffer between more intense commercial use districts and *residential* districts.

**Dimensional Standards**

**Minimum district size**

* Single family dwelling: 3,000 square feet (may be reduced to 2,000 square feet if common open space is provided.
* Multiple family dwelling: as required to comply with gross density factor.

**Maximum height**: 36

**Minimum setbacks:**

Non-residential uses: Street 10; side 5, rear 10

Residential uses: Street 7; side 5 (10 on upper stories); rear 15 or 20% of the average depth dimension of lot, whichever is less

**Max lot cover**:

Non-residential uses: 60

Residential uses: 40

**Open Space Requirements:**

Single-Family Where the *lot* size is between two thousand (2,000) and four thousand (4,000) square feet, qualifying *common open space* is required in an amount such that the sum of the square footage of the *lots* in the *development* plus the sum of the square footage for *common open space*, all divided by the number of single *family* *lots*, equals no less than four thousand (4,000) square feet.

Multiple-Family Qualifying *common open space* is required at a minimum of two hundred fifty (250) square feet per unit.

Non-Residential The minimum dimension for *nonresidential open space* shall be 10 feet and cover a minimum of 300 square feet, unless the area is a component of interior parking *landscape* and meets the requirements for *open space* credits for *water harvesting* described in 14-7.5(D)(6).

The percentage of *required open space* shall be calculated on the basis of total *lot* area, and shall be no less than 25% unless the conditions described in 14-7.5(D)(6) are met; then the *required open space* may be reduced by a maximum of 10% of the total *lot* size.